**Form 6 – Version 5.3**

*Survey and Mapping Infrastructure Act 2003*

## PERMANENT SURVEY MARK PLAN

| **REGISTERED NO.** |   |
| --- | --- |

| Bearings are |   | Distances are metres |
| --- | --- | --- |

| Picture for formatting purposes |
| --- |

| ***Mark Type:*** |   |   |
| --- | --- | --- |

| Suited to GNSS? | **DETAILS ON REVERSE COMPLETED:** [ ]  |
| --- | --- |
|   | Prepared by: |   | Date |   |
|  |  | (registered person or public authority) |  |  |

This form is to be completed in accordance with the Department’s Specification *Completion of Permanent Survey Mark Plans*

**Survey Control Register - Permanent Survey Mark Data Sheet**

| **REGISTERED NO.** |   |
| --- | --- |

| ***Administrative Data*** |
| --- |
| Alternative Name 1: |   | \*Installed by: |   |
| Alternative Name 2: |   | \*Date installed: |   |
| Alternative Name 3: |   | Date last visited: |   |
| \*Mark type: |   | \*Locality: |   |
|  |   | City or Town: |   |
| \*Mark condition: |   | \*Local government: |   |
| Location description: |   |
| Note: The Survey Control Register is the authoritative source for coordinate and height information.The vertical and horizontal data below **may not be** the current information regarding this mark. |
| ***Vertical Control Data*** |
| \*Height: |   | \*Datum: |   | Vertical Accuracy - \*Order: |   | \*Class: |   |
|  |
| Vertical Origin - \*Regd No: |   | \*Height: |   | \*Datum: |   |
|  |
| Geo-Sphd N: |   | Datum: |   | Model: |   |
|  |
| \*Fixed By: |   | \*Date: |   |  |
| ***Horizontal Control Data*** |
| \*Latitude: |  ° ′ ″ | \*Longitude: |  ° ′ ″ | \*Datum: |   |
|  |
| \*Easting: |   | \*Northing: |   | \*Zone: |   |
|  |
| \*Horiz Positional Uncertainty: |   | \*Fixed By: |   | \*Date: |   |
|  |
| #Horiz Origin Regd No: |   |  |
| #Latitude: |  ° ′ ″ | #Longitude: |  ° ′ ″ | #Datum: |   |
| ***Cadastral Connection Data*** |
| \*Connected on Cadastral Plan No.: |   |
| **Comments** |
|   |
|  |
| **Details completed by:**  | **Name:** |   | **Date:** |   |
|  | **Organisation:** |   |

\* Items marked thus are mandatory items for the section
# Items marked thus are mandatory items if the coordinates are determined by connection to an existing mark (i.e. not Network RTK or AUSPOS)